# Changelog since v0.4.1
- ⬆️ Update adafruit-circuitpython-ahtx0 to v1.0.25 (#149)

Co-authored-by: renovate[bot] <29139614+renovate[bot]@users.noreply.github.com> 
- ⬆️ Update adafruit-circuitpython-mcp230xx to v2.5.16 (#147)

Co-authored-by: renovate[bot] <29139614+renovate[bot]@users.noreply.github.com> 
- ⬆️ Update adafruit-circuitpython-ahtx0 to v1.0.24 (#146)

Co-authored-by: renovate[bot] <29139614+renovate[bot]@users.noreply.github.com> 
- ⬆️ Update alpine_3_19/git to v2.43.6-r0 (#145)

Co-authored-by: renovate[bot] <29139614+renovate[bot]@users.noreply.github.com> 
- ⬆️ Update gpiod to v2.2.3 (#144)

Co-authored-by: renovate[bot] <29139614+renovate[bot]@users.noreply.github.com> 
- ⬆️ Update Python to v3.11.11-r0 (#143)

Co-authored-by: renovate[bot] <29139614+renovate[bot]@users.noreply.github.com> 
- ⬆️ Update gpiod to v2.2.2 (#140)

Co-authored-by: renovate[bot] <29139614+renovate[bot]@users.noreply.github.com> 
- ⬆️ Update adafruit-circuitpython-ahtx0 to v1.0.23 
- ⬆️ Update smbus2 to v0.5.0 
- ⬆️ Update adafruit-circuitpython-mcp230xx to v2.5.15 
- ⬆️ Update adafruit-circuitpython-mcp230xx to v2.5.14 
- ⬆️ Update adafruit-circuitpython-ahtx0 to v1.0.22 
- ⬆️ Update alpine_3_19/git to v2.43.5-r0 
- ⬆️ Update Python to v3.11.10-r0 (#129)

Co-authored-by: renovate[bot] <29139614+renovate[bot]@users.noreply.github.com> 
- ⬆️ Update Python to v3.11.9-r1 
- ⬆️ Update gpiod to v2.2.1 
- ⬆️ Update gpiod to v2.2.0 
- ⬆️ Pin paho-mqtt to ==1.6.1 (#122)

Co-authored-by: renovate[bot] <29139614+renovate[bot]@users.noreply.github.com> 
